1. In the AddTwo program, what is the meaning of the INCLUDE directive?
   1. Copy necessary definitions and setup information from the Irvine32.inc txt file. The data from this file are inserted into the data stream read by the assembler
2. In the AddTwo program, what does the .CODE directive identify?
   1. The .CODE directive marks the beginning of the code segment
3. What are the names of the two segments in the AddTwo program?
   1. Code and Data
4. In the AddTwo program, which register holds the sum?
   1. EAX
5. In the AddTwo program, which statement halts the program?
   1. INVOKE ExitProcess,0